

|  |  |
| --- | --- |
| **CONVERSION OF THE VEHICLE: TOYOTA HIACE HIGH ROOF AMBULANCE** | |
| **A** | **PATIENT COMPARTMENT FITTINGS** |
| 1 | Insulation and covering of the patient compartment |
| 2 | Partition with sliding glass window for communication. |
| 3 | Cabinet for medical equipment & oxygen cylinders - Material: PVC |
| 4 | Flooring made with marine grade plywood - 18 mm thick, sturdy non-slip, anti-static and liquid-resistant vinyl. |
| 5 | Squad bench with under seat storage, backrest and seat belt - Capacity: 3- 4 persons |
| 6 | Doctor Seat with Fixed backrest, Swiveling Mechanism, 3 point Automatic Safety belt |
| **B** | **ELECTRICAL SYSTEM & COMPONENTS** |
| 7 | Electric wiring with insulation |
| 8 | Electric control panel/fuse box |
| 9 | 2x Socket 12V & 2x Outlet 220V |
| 10 | Shore line with connection cable 15m and 220V oulet |
| 11 | Roof type ventilation fan |
| 12 | Reverse Alarm |
| 13 | Video Recorder |
| 14 | Air conditioning unit for the patient compartment |
| 15 | Engine Heater |
| **C** | **LIGHTING SYSTEM** |
| 16 | LED lighting for the patient compartment |
| 17 | LED light bar with siren, speaker and microphone (color:as per customer requirements) |
| 18 | Strobe lights at the back of the vehicle (color:as per customer requirements) |
| 19 | Loading LED light |
| 20 | Flexible LED Light |
| **D** | **OXYGEN SYSTEM** |
| 21 | 2x 10L Oxygen cylinder, regulator, outlet, flow meter humidifier and oxygen mask |
| 22 | Oxygen system related hoses |
| **E** | **PATIENT TRANSPORT EQUIPMENT** |
| 23 | Automatic Loading Stretcher (CE Certified) |
| 24 | 2 Nos. Foldable Stretcher (CE Certified) |
| 25 | Spinal Board Long with head Immobilizer (CE Certified) |
| 26 | Stair Chair (CE Certified) |
| 27 | Fracture Splint (CE Certified) |
| 28 | Cervical Collar (CE Certified) |
| **F** | **MEDICAL EQUIPMENT** |
| 29 | First Aid Kit - 25 person (CE Certified) |
| 30 | Wall Mounted Sphygmomanometer (CE Certified) |
| 31 | Aneroid Sphygmomanometer (CE Certified) |
| 32 | Stethoscope Dual Head (CE Certified) |
| 33 | Syringes 3ml, 5ml, 10ml - Boxes (CE Certified) |
| 34 | 20L Portable Suction Machine PMSA - 3A/Canada (CE Certified) |
| 35 | AED Defibrillator HR-501 - Radian/South Korea (CE Certified) |
| 36 | ECG Machine, 3 Channel E3 - 3A/Canada (CE Certified) |
| 37 | BT-710 Pulse Oximeter Handheld woth Pediatric SPO2 Sensor - Bistos/South Korea (CE Certified) |
| 38 | GM620 Blood Glucose Meter with Test Strips - Bionime/USA (CE Certified) |
| 39 | UV Germicidal Lamp (CE Certified) |
| 40 | Heating Blanket (CE Certified) |
| 41 | Obstetric Kit (CE Certified) |
| 42 | Anti-epidemic Kit/PPE Kit (CE Certified) |
| **G** | **OTHER ACCESSORIES** |
| 43 | Fire Extinguisher 2kg |
| 44 | Emergency Hammer with Seat Belt Cutter |
| 45 | Emergency Portable Lantern/Light |
| 46 | Side Reflective Lines |
| 47 | All Text and Logos |



|  |  |
| --- | --- |
| 48 | Glass Tinting |
| 49 | 2 Nos. IV Hooks |
| 50 | Sharps Container |
| 51 | Class B Medical Waste Container 10L |
| 52 | Safe Locker with keys |

**TOYOTA HIACE HIGH ROOF AMBULANCE (AFTER PRODUCTION)**



# EXTERIOR

*NOTE: PHOTOS SHOWN ARE FOR REFERENCE ONLY. FINAL PRODUCTION WILL BE BASED ON CLIENT'S REQUEST.*



# INTERIOR

*NOTE: PHOTOS SHOWN ARE FOR REFERENCE ONLY. FINAL PRODUCTION WILL BE BASED ON CLIENT'S REQUEST.*